1911/2011 precision build class tool list

This course is designed to present coverage of modifications to the Colt type 1911 auto pistols, as used in Bullseye, Carry, Open or Stock competition. The student will learn different types of compensator systems as well as ergonomic enhancement techniques to fine-tune the Colt 1911 to any specifications. Precise barrel installation for maximum accuracy and detailed trigger work will be strongly emphasized.

***It is YOUR responsibility to follow all applicable laws and regulations pertaining to possessing, manufacturing and/or modifying a firearm.***

*We are not allowing any 80% frames or 1911 build kits.* It is recommended you bring a factory firearm and purchase a quality oversized/gunsmith fit barrel, and preferably a gunsmith fit bushing. The instructor will go over all the aftermarket upgrades, as well as the different types of competition configurations.  The more high end quality parts you can purchase, the more you will get from the fitting and customizing. If anyone has any questions that haven't already been covered, feel free to contact the instructor Rick Kennedy at swguntech@gmail.com

**Tool list**

8 oz ball peen hammer

pin punch set

basic screwdriver set

needle file set

Various files that you are comfortable with, flat, triangle, round, chainsaw with file handles

1911 bushing wrench

Square ½ inch india stones fine and medium

Square ¼ inch ceramic stone

Foredom or dremel tool with basic sanding/grinding/polishing and cut off bits

5mm 4 flute carbide end mill

dovetail cutter for sights of choice(if you purchased a bald slide)

 .330x65 Novak Front

 .359x60 Bomar Rear

 .495x65 Novak Rear

 .300x60 Wilson Front

Sandpaper in 240, 320, 400, 600 grit

Quality Oil

The instructor will be bringing a huge accompaniment of fixtures and gadgets that we currently use in the custom building circles for use in the class.